1 Questions
Thursday, 12 July 2018
8:11 AM
Are any of the resistors measured in Table 2-1 out of tolerance?

Answer:



You suspect that the percent difference between color-code and measured values could be due to an error in the meter. How could you find out if you are correct?

Answer:



Determine the four-band resistor color-code for the following resistors. The tolerance is 10%.

a)
12 Ω
b)
6.8 kΩ
c)
910 Ω
d)
4.7 MΩ
e)
1.0 Ω
Determine the expected value for resistors with the following color-codes:

a)
red-red-black-gold
b)
violet-green-brown-silver
c)
green-brown-brown-gold
d)
white-brown-gold-gold
e)
gray-red-yellow-silver
A resistor is color coded: red-violet-orange-gold.
a)
What is the largest value the resistor can be and still be in tolerance?
b)
What is the smallest value?