1 Questions
Thursday, 12 July 2018
8:11 AM
Compare the voltage difference calculation in Table 3-3 through Table 3-6. Does the circuit's reference point (common) have any effect on the voltage differences across any of the resistors? Explain your answer.

Answer:



Define the term common.

Answer:



If you measured 𝑉𝐴𝐵 as 12.0 V, what is 𝑉𝐵𝐴?

Answer:
Suppose 𝑉𝑀=−220 V and 𝑉𝑁=−150 V. What is 𝑉𝑀𝑁?
Answer:
If a test point in a circuit is marked +5.0 V and a second test point is marked -3.3 V, what voltage reading would you expect on a voltmeter connected between the two test points? Assume the reference lead on the meter is at the lowest potential.
Answer: