Answer:
Answer:


Compare the measured voltages in Tables 4-10 and 4-11. What conclusion can you draw about the two circuits?
Answer:


Compute the load current you would expect to measure if the load resistor in Figure 4-11 were replaced with a short. Then repeat the computation for the Thévenin circuit you drew in step 10.
Draw the Thévenin equivalent circuit for the circuits shown below.
Figure 4-13
Figure 4-13(a) shows a circuit, and Figure 4-13(b) shows its equivalent Thévenin circuit. Explain why  𝑅1 has no effect on the Thévenin circuit.
What advantage does Thévenin's theorem offer for computing the load voltage across each of the load resistors tested in this experiment?